Patch taken from upstream MR
https://gitlab.freedesktop.org/xorg/xserver/-/merge_requests/1006 -- merged,
but not yet included in a release.

A minor edit to the ABI_VIDEODRV_VERSION hunk was needed to apply to 21.1.21.


diff --git a/dix/pixmap.c b/dix/pixmap.c
index 5a0146bbb667a07bee5b53ff5390e435976d2d4b..0b01c4ee0640677fbd2f2fff36ad1517135e0a4e 100644
--- a/dix/pixmap.c
+++ b/dix/pixmap.c
@@ -262,12 +262,11 @@ PixmapStopDirtyTracking(DrawablePtr src, PixmapPtr secondary_dst)
     return TRUE;
 }
 
-static void
-PixmapDirtyCopyArea(PixmapPtr dst,
-                    PixmapDirtyUpdatePtr dirty,
+void
+PixmapDirtyCopyArea(PixmapPtr dst, DrawablePtr src,
+                    int x, int y, int dst_x, int dst_y,
                     RegionPtr dirty_region)
 {
-    DrawablePtr src = dirty->src;
     ScreenPtr pScreen = src->pScreen;
     int n;
     BoxPtr b;
@@ -294,9 +293,8 @@ PixmapDirtyCopyArea(PixmapPtr dst,
         h = dst_box.y2 - dst_box.y1;
 
         pGC->ops->CopyArea(src, &dst->drawable, pGC,
-                           dirty->x + dst_box.x1, dirty->y + dst_box.y1, w, h,
-                           dirty->dst_x + dst_box.x1,
-                           dirty->dst_y + dst_box.y1);
+                           x + dst_box.x1, y + dst_box.y1, w, h,
+                           dst_x + dst_box.x1, dst_y + dst_box.y1);
         b++;
     }
     FreeScratchGC(pGC);
@@ -408,7 +406,8 @@ Bool PixmapSyncDirtyHelper(PixmapDirtyUpdatePtr dirty)
     RegionTranslate(&pixregion, -dirty->x, -dirty->y);
 
     if (!pScreen->root || dirty->rotation == RR_Rotate_0)
-        PixmapDirtyCopyArea(dst, dirty, &pixregion);
+        PixmapDirtyCopyArea(dst, dirty->src, dirty->x, dirty->y,
+                            dirty->dst_x, dirty->dst_y, &pixregion);
     else
         PixmapDirtyCompositeRotate(dst, dirty, &pixregion);
     pScreen->SourceValidate = SourceValidate;
diff --git a/hw/xfree86/common/xf86Module.h b/hw/xfree86/common/xf86Module.h
index 33cf0e56a45b0202ab45cfc86538fd43e550fc80..c59e53a55c68f1a55262e3b85865192e68380a5f 100644
--- a/hw/xfree86/common/xf86Module.h
+++ b/hw/xfree86/common/xf86Module.h
@@ -74,7 +74,7 @@
  * mask is 0xFFFF0000.
  */
 #define ABI_ANSIC_VERSION	SET_ABI_VERSION(0, 4)
-#define ABI_VIDEODRV_VERSION	SET_ABI_VERSION(25, 2)
+#define ABI_VIDEODRV_VERSION	SET_ABI_VERSION(25, 4)
 #define ABI_XINPUT_VERSION	SET_ABI_VERSION(24, 4)
 #define ABI_EXTENSION_VERSION	SET_ABI_VERSION(10, 0)
 
diff --git a/hw/xfree86/drivers/modesetting/driver.c b/hw/xfree86/drivers/modesetting/driver.c
index fe3315a9c49cfdb545f062e77db46fc2e3dcc42e..7a7d5c3887fcf226347582c3c3482ab395aa04e3 100644
--- a/hw/xfree86/drivers/modesetting/driver.c
+++ b/hw/xfree86/drivers/modesetting/driver.c
@@ -145,6 +145,7 @@ static const OptionInfoRec Options[] = {
     {OPTION_VARIABLE_REFRESH, "VariableRefresh", OPTV_BOOLEAN, {0}, FALSE},
     {OPTION_USE_GAMMA_LUT, "UseGammaLUT", OPTV_BOOLEAN, {0}, FALSE},
     {OPTION_ASYNC_FLIP_SECONDARIES, "AsyncFlipSecondaries", OPTV_BOOLEAN, {0}, FALSE},
+    {OPTION_TEARFREE, "TearFree", OPTV_BOOLEAN, {0}, FALSE},
     {-1, NULL, OPTV_NONE, {0}, FALSE}
 };
 
@@ -548,14 +549,16 @@ rotate_clip(PixmapPtr pixmap, BoxPtr rect, drmModeClip *clip, Rotation rotation)
 }
 
 static int
-dispatch_dirty_region(ScrnInfoPtr scrn, xf86CrtcPtr crtc,
-		      PixmapPtr pixmap, DamagePtr damage, int fb_id)
+dispatch_damages(ScrnInfoPtr scrn, xf86CrtcPtr crtc, RegionPtr dirty,
+                 PixmapPtr pixmap, DamagePtr damage, int fb_id)
 {
     modesettingPtr ms = modesettingPTR(scrn);
-    RegionPtr dirty = DamageRegion(damage);
     unsigned num_cliprects = REGION_NUM_RECTS(dirty);
     int ret = 0;
 
+    if (!ms->dirty_enabled)
+        return 0;
+
     if (num_cliprects) {
         drmModeClip *clip = xallocarray(num_cliprects, sizeof(drmModeClip));
         BoxPtr rect = REGION_RECTS(dirty);
@@ -579,12 +582,102 @@ dispatch_dirty_region(ScrnInfoPtr scrn, xf86CrtcPtr crtc,
             }
         }
 
+        if (ret == -EINVAL || ret == -ENOSYS) {
+            xf86DrvMsg(scrn->scrnIndex, X_INFO,
+                       "Disabling kernel dirty updates, not required.\n");
+            ms->dirty_enabled = FALSE;
+        }
+
         free(clip);
-        DamageEmpty(damage);
+        if (damage)
+            DamageEmpty(damage);
     }
     return ret;
 }
 
+static int
+dispatch_dirty_region(ScrnInfoPtr scrn, xf86CrtcPtr crtc,
+                      PixmapPtr pixmap, DamagePtr damage, int fb_id)
+{
+    return dispatch_damages(scrn, crtc, DamageRegion(damage),
+                            pixmap, damage, fb_id);
+}
+
+static void
+ms_tearfree_update_damages(ScreenPtr pScreen)
+{
+    ScrnInfoPtr scrn = xf86ScreenToScrn(pScreen);
+    xf86CrtcConfigPtr xf86_config = XF86_CRTC_CONFIG_PTR(scrn);
+    modesettingPtr ms = modesettingPTR(scrn);
+    RegionPtr dirty = DamageRegion(ms->damage);
+    int c, i;
+
+    if (RegionNil(dirty))
+        return;
+
+    for (c = 0; c < xf86_config->num_crtc; c++) {
+        xf86CrtcPtr crtc = xf86_config->crtc[c];
+        drmmode_crtc_private_ptr drmmode_crtc = crtc->driver_private;
+        drmmode_tearfree_ptr trf = &drmmode_crtc->tearfree;
+        RegionRec region;
+
+        /* Compute how much of the damage intersects with this CRTC */
+        RegionInit(&region, &crtc->bounds, 0);
+        RegionIntersect(&region, &region, dirty);
+
+        if (trf->buf[0].px) {
+            for (i = 0; i < ARRAY_SIZE(trf->buf); i++)
+                RegionUnion(&trf->buf[i].dmg, &trf->buf[i].dmg, &region);
+        } else {
+            /* Just notify the kernel of the damages if TearFree isn't used */
+            dispatch_damages(scrn, crtc, &region,
+                             pScreen->GetScreenPixmap(pScreen),
+                             NULL, ms->drmmode.fb_id);
+        }
+    }
+    DamageEmpty(ms->damage);
+}
+
+static void
+ms_tearfree_do_flips(ScreenPtr pScreen)
+{
+#ifdef GLAMOR_HAS_GBM
+    ScrnInfoPtr scrn = xf86ScreenToScrn(pScreen);
+    xf86CrtcConfigPtr xf86_config = XF86_CRTC_CONFIG_PTR(scrn);
+    modesettingPtr ms = modesettingPTR(scrn);
+    int c;
+
+    if (!ms->drmmode.tearfree_enable)
+        return;
+
+    for (c = 0; c < xf86_config->num_crtc; c++) {
+        xf86CrtcPtr crtc = xf86_config->crtc[c];
+        drmmode_crtc_private_ptr drmmode_crtc = crtc->driver_private;
+        drmmode_tearfree_ptr trf = &drmmode_crtc->tearfree;
+
+        /* Skip disabled CRTCs and those which aren't using TearFree */
+        if (!trf->buf[0].px || !crtc->scrn->vtSema || !xf86_crtc_on(crtc))
+            continue;
+
+        /* Skip if the last flip is still pending, a DRI client is flipping, or
+         * there isn't any damage on the front buffer.
+         */
+        if (trf->flip_seq || ms->drmmode.dri2_flipping ||
+            ms->drmmode.present_flipping ||
+            RegionNil(&trf->buf[trf->back_idx ^ 1].dmg))
+            continue;
+
+        /* Flip. If it fails, notify the kernel of the front buffer damages */
+        if (ms_do_tearfree_flip(pScreen, crtc)) {
+            dispatch_damages(scrn, crtc, &trf->buf[trf->back_idx ^ 1].dmg,
+                             trf->buf[trf->back_idx ^ 1].px, NULL,
+                             trf->buf[trf->back_idx ^ 1].fb_id);
+            RegionEmpty(&trf->buf[trf->back_idx ^ 1].dmg);
+        }
+    }
+#endif
+}
+
 static void
 dispatch_dirty(ScreenPtr pScreen)
 {
@@ -606,12 +699,9 @@ dispatch_dirty(ScreenPtr pScreen)
 
         ret = dispatch_dirty_region(scrn, crtc, pixmap, ms->damage, fb_id);
         if (ret == -EINVAL || ret == -ENOSYS) {
-            ms->dirty_enabled = FALSE;
             DamageUnregister(ms->damage);
             DamageDestroy(ms->damage);
             ms->damage = NULL;
-            xf86DrvMsg(scrn->scrnIndex, X_INFO,
-                       "Disabling kernel dirty updates, not required.\n");
             return;
         }
     }
@@ -742,10 +832,13 @@ msBlockHandler(ScreenPtr pScreen, void *timeout)
     pScreen->BlockHandler = msBlockHandler;
     if (pScreen->isGPU && !ms->drmmode.reverse_prime_offload_mode)
         dispatch_secondary_dirty(pScreen);
+    else if (ms->drmmode.tearfree_enable)
+        ms_tearfree_update_damages(pScreen);
     else if (ms->dirty_enabled)
         dispatch_dirty(pScreen);
 
     ms_dirty_update(pScreen, timeout);
+    ms_tearfree_do_flips(pScreen);
 }
 
 static void
@@ -1281,6 +1374,27 @@ PreInit(ScrnInfoPtr pScrn, int flags)
         ms->atomic_modeset = FALSE;
     }
 
+    /* TearFree requires glamor and, if PageFlip is enabled, universal planes */
+    if (xf86ReturnOptValBool(ms->drmmode.Options, OPTION_TEARFREE, FALSE)) {
+        if (pScrn->is_gpu) {
+            xf86DrvMsg(pScrn->scrnIndex, X_WARNING,
+                       "TearFree cannot synchronize PRIME; use 'PRIME Synchronization' instead\n");
+        } else if (ms->drmmode.glamor) {
+            /* Atomic modesetting implicitly enables universal planes */
+            if (!ms->drmmode.pageflip || ms->atomic_modeset ||
+                !drmSetClientCap(ms->fd, DRM_CLIENT_CAP_UNIVERSAL_PLANES, 1)) {
+                ms->drmmode.tearfree_enable = TRUE;
+                xf86DrvMsg(pScrn->scrnIndex, X_INFO, "TearFree: enabled\n");
+            } else {
+                xf86DrvMsg(pScrn->scrnIndex, X_WARNING,
+                           "TearFree requires either universal planes, or setting 'Option \"PageFlip\" \"off\"'\n");
+            }
+        } else {
+            xf86DrvMsg(pScrn->scrnIndex, X_WARNING,
+                       "TearFree requires Glamor acceleration\n");
+        }
+    }
+
     ms->kms_has_modifiers = FALSE;
     ret = drmGetCap(ms->fd, DRM_CAP_ADDFB2_MODIFIERS, &value);
     if (ret == 0 && value != 0)
@@ -1628,13 +1742,13 @@ CreateScreenResources(ScreenPtr pScreen)
 
     err = drmModeDirtyFB(ms->fd, ms->drmmode.fb_id, NULL, 0);
 
-    if (err != -EINVAL && err != -ENOSYS) {
+    if ((err != -EINVAL && err != -ENOSYS) || ms->drmmode.tearfree_enable) {
         ms->damage = DamageCreate(NULL, NULL, DamageReportNone, TRUE,
                                   pScreen, rootPixmap);
 
         if (ms->damage) {
             DamageRegister(&rootPixmap->drawable, ms->damage);
-            ms->dirty_enabled = TRUE;
+            ms->dirty_enabled = err != -EINVAL && err != -ENOSYS;
             xf86DrvMsg(pScrn->scrnIndex, X_INFO, "Damage tracking initialized\n");
         }
         else {
diff --git a/hw/xfree86/drivers/modesetting/driver.h b/hw/xfree86/drivers/modesetting/driver.h
index 71aa8730ec2fd74bec50d2bf237b474abe5197df..3f2b1d1aef4170793a4c2bfd18543130ef5aa34f 100644
--- a/hw/xfree86/drivers/modesetting/driver.h
+++ b/hw/xfree86/drivers/modesetting/driver.h
@@ -61,6 +61,7 @@ typedef enum {
     OPTION_VARIABLE_REFRESH,
     OPTION_USE_GAMMA_LUT,
     OPTION_ASYNC_FLIP_SECONDARIES,
+    OPTION_TEARFREE,
 } modesettingOpts;
 
 typedef struct
@@ -86,10 +87,13 @@ struct ms_drm_queue {
     struct xorg_list list;
     xf86CrtcPtr crtc;
     uint32_t seq;
+    uint64_t msc;
     void *data;
     ScrnInfoPtr scrn;
     ms_drm_handler_proc handler;
     ms_drm_abort_proc abort;
+    Bool kernel_queued;
+    Bool aborted;
 };
 
 typedef struct _modesettingRec {
@@ -238,6 +242,8 @@ Bool ms_do_pageflip(ScreenPtr screen,
                     ms_pageflip_abort_proc pageflip_abort,
                     const char *log_prefix);
 
+Bool ms_do_tearfree_flip(ScreenPtr screen, xf86CrtcPtr crtc);
+
 #endif
 
 int ms_flush_drm_events(ScreenPtr screen);
diff --git a/hw/xfree86/drivers/modesetting/drmmode_display.c b/hw/xfree86/drivers/modesetting/drmmode_display.c
index 65e8e63353a04693de76fba1c808c8bfcfd63676..8f8e4060a9fc27c4dbc7b82c4fa01f9fbbb8463c 100644
--- a/hw/xfree86/drivers/modesetting/drmmode_display.c
+++ b/hw/xfree86/drivers/modesetting/drmmode_display.c
@@ -632,6 +632,7 @@ drmmode_crtc_get_fb_id(xf86CrtcPtr crtc, uint32_t *fb_id, int *x, int *y)
 {
     drmmode_crtc_private_ptr drmmode_crtc = crtc->driver_private;
     drmmode_ptr drmmode = drmmode_crtc->drmmode;
+    drmmode_tearfree_ptr trf = &drmmode_crtc->tearfree;
     int ret;
 
     *fb_id = 0;
@@ -646,6 +647,10 @@ drmmode_crtc_get_fb_id(xf86CrtcPtr crtc, uint32_t *fb_id, int *x, int *y)
             *x = drmmode_crtc->prime_pixmap_x;
         *y = 0;
     }
+    else if (trf->buf[trf->back_idx ^ 1].px) {
+        *fb_id = trf->buf[trf->back_idx ^ 1].fb_id;
+        *x = *y = 0;
+    }
     else if (drmmode_crtc->rotate_fb_id) {
         *fb_id = drmmode_crtc->rotate_fb_id;
         *x = *y = 0;
@@ -922,6 +927,10 @@ drmmode_crtc_set_mode(xf86CrtcPtr crtc, Bool test_only)
     drmmode_ConvertToKMode(crtc->scrn, &kmode, &crtc->mode);
     ret = drmModeSetCrtc(drmmode->fd, drmmode_crtc->mode_crtc->crtc_id,
                          fb_id, x, y, output_ids, output_count, &kmode);
+    if (!ret && !ms->atomic_modeset) {
+        drmmode_crtc->src_x = x;
+        drmmode_crtc->src_y = y;
+    }
 
     drmmode_set_ctm(crtc, ctm);
 
@@ -930,7 +939,8 @@ drmmode_crtc_set_mode(xf86CrtcPtr crtc, Bool test_only)
 }
 
 int
-drmmode_crtc_flip(xf86CrtcPtr crtc, uint32_t fb_id, uint32_t flags, void *data)
+drmmode_crtc_flip(xf86CrtcPtr crtc, uint32_t fb_id, int x, int y,
+                  uint32_t flags, void *data)
 {
     modesettingPtr ms = modesettingPTR(crtc->scrn);
     drmmode_crtc_private_ptr drmmode_crtc = crtc->driver_private;
@@ -942,7 +952,7 @@ drmmode_crtc_flip(xf86CrtcPtr crtc, uint32_t fb_id, uint32_t flags, void *data)
         if (!req)
             return 1;
 
-        ret = plane_add_props(req, crtc, fb_id, crtc->x, crtc->y);
+        ret = plane_add_props(req, crtc, fb_id, x, y);
         flags |= DRM_MODE_ATOMIC_NONBLOCK;
         if (ret == 0)
             ret = drmModeAtomicCommit(ms->fd, req, flags, data);
@@ -950,6 +960,26 @@ drmmode_crtc_flip(xf86CrtcPtr crtc, uint32_t fb_id, uint32_t flags, void *data)
         return ret;
     }
 
+    /* The frame buffer source coordinates may change when switching between the
+     * primary frame buffer and a per-CRTC frame buffer. Set the correct source
+     * coordinates if they differ for this flip.
+     */
+    if (drmmode_crtc->src_x != x || drmmode_crtc->src_y != y) {
+        ret = drmModeSetPlane(ms->fd, drmmode_crtc->plane_id,
+                              drmmode_crtc->mode_crtc->crtc_id, fb_id, 0,
+                              0, 0, crtc->mode.HDisplay, crtc->mode.VDisplay,
+                              x << 16, y << 16, crtc->mode.HDisplay << 16,
+                              crtc->mode.VDisplay << 16);
+        if (ret) {
+            xf86DrvMsg(crtc->scrn->scrnIndex, X_WARNING,
+                       "error changing fb src coordinates for flip: %d\n", ret);
+            return ret;
+        }
+
+        drmmode_crtc->src_x = x;
+        drmmode_crtc->src_y = y;
+    }
+
     return drmModePageFlip(ms->fd, drmmode_crtc->mode_crtc->crtc_id,
                            fb_id, flags, data);
 }
@@ -1548,6 +1578,90 @@ drmmode_copy_fb(ScrnInfoPtr pScrn, drmmode_ptr drmmode)
 #endif
 }
 
+void
+drmmode_copy_damage(xf86CrtcPtr crtc, PixmapPtr dst, RegionPtr dmg, Bool empty)
+{
+#ifdef GLAMOR_HAS_GBM
+    ScreenPtr pScreen = xf86ScrnToScreen(crtc->scrn);
+    DrawableRec *src;
+
+    /* Copy the screen's pixmap into the destination pixmap */
+    if (crtc->rotatedPixmap) {
+        src = &crtc->rotatedPixmap->drawable;
+        xf86RotateCrtcRedisplay(crtc, dst, src, dmg, FALSE);
+    } else {
+        src = &pScreen->GetScreenPixmap(pScreen)->drawable;
+        PixmapDirtyCopyArea(dst, src, 0, 0, -crtc->x, -crtc->y, dmg);
+    }
+
+    /* Reset the damages if requested */
+    if (empty)
+        RegionEmpty(dmg);
+
+    /* Wait until the GC operations finish */
+    modesettingPTR(crtc->scrn)->glamor.finish(pScreen);
+#endif
+}
+
+static void
+drmmode_shadow_fb_destroy(xf86CrtcPtr crtc, PixmapPtr pixmap,
+                          void *data, drmmode_bo *bo, uint32_t *fb_id);
+static void
+drmmode_destroy_tearfree_shadow(xf86CrtcPtr crtc)
+{
+    drmmode_crtc_private_ptr drmmode_crtc = crtc->driver_private;
+    drmmode_tearfree_ptr trf = &drmmode_crtc->tearfree;
+    int i;
+
+    if (trf->flip_seq)
+        ms_drm_abort_seq(crtc->scrn, trf->flip_seq);
+
+    for (i = 0; i < ARRAY_SIZE(trf->buf); i++) {
+        if (trf->buf[i].px) {
+            drmmode_shadow_fb_destroy(crtc, trf->buf[i].px, (void *)(long)1,
+                                      &trf->buf[i].bo, &trf->buf[i].fb_id);
+            trf->buf[i].px = NULL;
+            RegionUninit(&trf->buf[i].dmg);
+        }
+    }
+}
+
+static PixmapPtr
+drmmode_shadow_fb_create(xf86CrtcPtr crtc, void *data, int width, int height,
+                         drmmode_bo *bo, uint32_t *fb_id);
+static Bool
+drmmode_create_tearfree_shadow(xf86CrtcPtr crtc)
+{
+    drmmode_crtc_private_ptr drmmode_crtc = crtc->driver_private;
+    drmmode_ptr drmmode = drmmode_crtc->drmmode;
+    drmmode_tearfree_ptr trf = &drmmode_crtc->tearfree;
+    uint32_t w = crtc->mode.HDisplay, h = crtc->mode.VDisplay;
+    int i;
+
+    if (!drmmode->tearfree_enable)
+        return TRUE;
+
+    /* Destroy the old mode's buffers and make new ones */
+    drmmode_destroy_tearfree_shadow(crtc);
+    for (i = 0; i < ARRAY_SIZE(trf->buf); i++) {
+        trf->buf[i].px = drmmode_shadow_fb_create(crtc, NULL, w, h,
+                                                  &trf->buf[i].bo,
+                                                  &trf->buf[i].fb_id);
+        if (!trf->buf[i].px) {
+            drmmode_destroy_tearfree_shadow(crtc);
+            xf86DrvMsg(crtc->scrn->scrnIndex, X_ERROR,
+                       "shadow creation failed for TearFree buf%d\n", i);
+            return FALSE;
+        }
+        RegionInit(&trf->buf[i].dmg, &crtc->bounds, 0);
+    }
+
+    /* Initialize the front buffer with the current scanout */
+    drmmode_copy_damage(crtc, trf->buf[trf->back_idx ^ 1].px,
+                        &trf->buf[trf->back_idx ^ 1].dmg, TRUE);
+    return TRUE;
+}
+
 static Bool
 drmmode_set_mode_major(xf86CrtcPtr crtc, DisplayModePtr mode,
                        Rotation rotation, int x, int y)
@@ -1581,6 +1695,10 @@ drmmode_set_mode_major(xf86CrtcPtr crtc, DisplayModePtr mode,
         crtc->funcs->gamma_set(crtc, crtc->gamma_red, crtc->gamma_green,
                                crtc->gamma_blue, crtc->gamma_size);
 
+        ret = drmmode_create_tearfree_shadow(crtc);
+        if (!ret)
+            goto done;
+
         can_test = drmmode_crtc_can_test_mode(crtc);
         if (drmmode_crtc_set_mode(crtc, can_test)) {
             xf86DrvMsg(crtc->scrn->scrnIndex, X_ERROR,
@@ -1626,6 +1744,7 @@ drmmode_set_mode_major(xf86CrtcPtr crtc, DisplayModePtr mode,
         crtc->y = saved_y;
         crtc->rotation = saved_rotation;
         crtc->mode = saved_mode;
+        drmmode_create_tearfree_shadow(crtc);
     } else
         crtc->active = TRUE;
 
@@ -1931,33 +2050,42 @@ drmmode_clear_pixmap(PixmapPtr pixmap)
 }
 
 static void *
-drmmode_shadow_allocate(xf86CrtcPtr crtc, int width, int height)
+drmmode_shadow_fb_allocate(xf86CrtcPtr crtc, int width, int height,
+                           drmmode_bo *bo, uint32_t *fb_id)
 {
     drmmode_crtc_private_ptr drmmode_crtc = crtc->driver_private;
     drmmode_ptr drmmode = drmmode_crtc->drmmode;
     int ret;
 
-    if (!drmmode_create_bo(drmmode, &drmmode_crtc->rotate_bo,
-                           width, height, drmmode->kbpp)) {
+    if (!drmmode_create_bo(drmmode, bo, width, height, drmmode->kbpp)) {
         xf86DrvMsg(crtc->scrn->scrnIndex, X_ERROR,
                "Couldn't allocate shadow memory for rotated CRTC\n");
         return NULL;
     }
 
-    ret = drmmode_bo_import(drmmode, &drmmode_crtc->rotate_bo,
-                            &drmmode_crtc->rotate_fb_id);
+    ret = drmmode_bo_import(drmmode, bo, fb_id);
 
     if (ret) {
         ErrorF("failed to add rotate fb\n");
-        drmmode_bo_destroy(drmmode, &drmmode_crtc->rotate_bo);
+        drmmode_bo_destroy(drmmode, bo);
         return NULL;
     }
 
 #ifdef GLAMOR_HAS_GBM
     if (drmmode->gbm)
-        return drmmode_crtc->rotate_bo.gbm;
+        return bo->gbm;
 #endif
-    return drmmode_crtc->rotate_bo.dumb;
+    return bo->dumb;
+}
+
+static void *
+drmmode_shadow_allocate(xf86CrtcPtr crtc, int width, int height)
+{
+    drmmode_crtc_private_ptr drmmode_crtc = crtc->driver_private;
+
+    return drmmode_shadow_fb_allocate(crtc, width, height,
+                                      &drmmode_crtc->rotate_bo,
+                                      &drmmode_crtc->rotate_fb_id);
 }
 
 static PixmapPtr
@@ -1983,70 +2111,91 @@ static Bool
 drmmode_set_pixmap_bo(drmmode_ptr drmmode, PixmapPtr pixmap, drmmode_bo *bo);
 
 static PixmapPtr
-drmmode_shadow_create(xf86CrtcPtr crtc, void *data, int width, int height)
+drmmode_shadow_fb_create(xf86CrtcPtr crtc, void *data, int width, int height,
+                         drmmode_bo *bo, uint32_t *fb_id)
 {
     ScrnInfoPtr scrn = crtc->scrn;
     drmmode_crtc_private_ptr drmmode_crtc = crtc->driver_private;
     drmmode_ptr drmmode = drmmode_crtc->drmmode;
-    uint32_t rotate_pitch;
-    PixmapPtr rotate_pixmap;
+    uint32_t pitch;
+    PixmapPtr pixmap;
     void *pPixData = NULL;
 
     if (!data) {
-        data = drmmode_shadow_allocate(crtc, width, height);
+        data = drmmode_shadow_fb_allocate(crtc, width, height, bo, fb_id);
         if (!data) {
             xf86DrvMsg(scrn->scrnIndex, X_ERROR,
-                       "Couldn't allocate shadow pixmap for rotated CRTC\n");
+                       "Couldn't allocate shadow pixmap for CRTC\n");
             return NULL;
         }
     }
 
-    if (!drmmode_bo_has_bo(&drmmode_crtc->rotate_bo)) {
+    if (!drmmode_bo_has_bo(bo)) {
         xf86DrvMsg(scrn->scrnIndex, X_ERROR,
-                   "Couldn't allocate shadow pixmap for rotated CRTC\n");
+                   "Couldn't allocate shadow pixmap for CRTC\n");
         return NULL;
     }
 
-    pPixData = drmmode_bo_map(drmmode, &drmmode_crtc->rotate_bo);
-    rotate_pitch = drmmode_bo_get_pitch(&drmmode_crtc->rotate_bo);
+    pPixData = drmmode_bo_map(drmmode, bo);
+    pitch = drmmode_bo_get_pitch(bo);
 
-    rotate_pixmap = drmmode_create_pixmap_header(scrn->pScreen,
-                                                 width, height,
-                                                 scrn->depth,
-                                                 drmmode->kbpp,
-                                                 rotate_pitch,
-                                                 pPixData);
+    pixmap = drmmode_create_pixmap_header(scrn->pScreen,
+                                          width, height,
+                                          scrn->depth,
+                                          drmmode->kbpp,
+                                          pitch,
+                                          pPixData);
 
-    if (rotate_pixmap == NULL) {
+    if (pixmap == NULL) {
         xf86DrvMsg(scrn->scrnIndex, X_ERROR,
-                   "Couldn't allocate shadow pixmap for rotated CRTC\n");
+                   "Couldn't allocate shadow pixmap for CRTC\n");
         return NULL;
     }
 
-    drmmode_set_pixmap_bo(drmmode, rotate_pixmap, &drmmode_crtc->rotate_bo);
+    drmmode_set_pixmap_bo(drmmode, pixmap, bo);
+
+    return pixmap;
+}
+
+static PixmapPtr
+drmmode_shadow_create(xf86CrtcPtr crtc, void *data, int width, int height)
+{
+    drmmode_crtc_private_ptr drmmode_crtc = crtc->driver_private;
 
-    return rotate_pixmap;
+    return drmmode_shadow_fb_create(crtc, data, width, height,
+                                    &drmmode_crtc->rotate_bo,
+                                    &drmmode_crtc->rotate_fb_id);
 }
 
 static void
-drmmode_shadow_destroy(xf86CrtcPtr crtc, PixmapPtr rotate_pixmap, void *data)
+drmmode_shadow_fb_destroy(xf86CrtcPtr crtc, PixmapPtr pixmap,
+                          void *data, drmmode_bo *bo, uint32_t *fb_id)
 {
     drmmode_crtc_private_ptr drmmode_crtc = crtc->driver_private;
     drmmode_ptr drmmode = drmmode_crtc->drmmode;
 
-    if (rotate_pixmap) {
-        rotate_pixmap->drawable.pScreen->DestroyPixmap(rotate_pixmap);
+    if (pixmap) {
+        pixmap->drawable.pScreen->DestroyPixmap(pixmap);
     }
 
     if (data) {
-        drmModeRmFB(drmmode->fd, drmmode_crtc->rotate_fb_id);
-        drmmode_crtc->rotate_fb_id = 0;
+        drmModeRmFB(drmmode->fd, *fb_id);
+        *fb_id = 0;
 
-        drmmode_bo_destroy(drmmode, &drmmode_crtc->rotate_bo);
-        memset(&drmmode_crtc->rotate_bo, 0, sizeof drmmode_crtc->rotate_bo);
+        drmmode_bo_destroy(drmmode, bo);
+        memset(bo, 0, sizeof(*bo));
     }
 }
 
+static void
+drmmode_shadow_destroy(xf86CrtcPtr crtc, PixmapPtr pixmap, void *data)
+{
+    drmmode_crtc_private_ptr drmmode_crtc = crtc->driver_private;
+
+    drmmode_shadow_fb_destroy(crtc, pixmap, data, &drmmode_crtc->rotate_bo,
+                              &drmmode_crtc->rotate_fb_id);
+}
+
 static void
 drmmode_crtc_destroy(xf86CrtcPtr crtc)
 {
@@ -2380,6 +2529,7 @@ drmmode_crtc_init(ScrnInfoPtr pScrn, drmmode_ptr drmmode, drmModeResPtr mode_res
     drmmode_crtc->drmmode = drmmode;
     drmmode_crtc->vblank_pipe = drmmode_crtc_vblank_pipe(num);
     xorg_list_init(&drmmode_crtc->mode_list);
+    drmmode_crtc->next_msc = UINT64_MAX;
 
     props = drmModeObjectGetProperties(drmmode->fd, mode_res->crtcs[num],
                                        DRM_MODE_OBJECT_CRTC);
@@ -4242,6 +4392,7 @@ drmmode_free_bos(ScrnInfoPtr pScrn, drmmode_ptr drmmode)
         drmmode_crtc_private_ptr drmmode_crtc = crtc->driver_private;
 
         dumb_bo_destroy(drmmode->fd, drmmode_crtc->cursor_bo);
+        drmmode_destroy_tearfree_shadow(crtc);
     }
 }
 
diff --git a/hw/xfree86/drivers/modesetting/drmmode_display.h b/hw/xfree86/drivers/modesetting/drmmode_display.h
index 2a9a915293a5ab092bd4de9749b795228a505b6f..145cb8cc7bac04da8f83d55dd85699523a4b873a 100644
--- a/hw/xfree86/drivers/modesetting/drmmode_display.h
+++ b/hw/xfree86/drivers/modesetting/drmmode_display.h
@@ -135,6 +135,7 @@ typedef struct {
     Bool async_flip_secondaries;
     Bool dri2_enable;
     Bool present_enable;
+    Bool tearfree_enable;
 
     uint32_t vrr_prop_id;
     Bool use_ctm;
@@ -166,6 +167,19 @@ typedef struct {
     uint64_t *modifiers;
 } drmmode_format_rec, *drmmode_format_ptr;
 
+typedef struct {
+    drmmode_bo bo;
+    uint32_t fb_id;
+    PixmapPtr px;
+    RegionRec dmg;
+} drmmode_shadow_fb_rec, *drmmode_shadow_fb_ptr;
+
+typedef struct {
+    drmmode_shadow_fb_rec buf[2];
+    uint32_t back_idx;
+    uint32_t flip_seq;
+} drmmode_tearfree_rec, *drmmode_tearfree_ptr;
+
 typedef struct {
     drmmode_ptr drmmode;
     drmModeCrtcPtr mode_crtc;
@@ -184,11 +198,14 @@ typedef struct {
 
     drmmode_bo rotate_bo;
     unsigned rotate_fb_id;
+    drmmode_tearfree_rec tearfree;
 
     PixmapPtr prime_pixmap;
     PixmapPtr prime_pixmap_back;
     unsigned prime_pixmap_x;
 
+    int src_x, src_y;
+
     /**
      * @{ MSC (vblank count) handling for the PRESENT extension.
      *
@@ -200,6 +217,8 @@ typedef struct {
     uint64_t msc_high;
     /** @} */
 
+    uint64_t next_msc;
+
     Bool need_modeset;
     struct xorg_list mode_list;
 
@@ -308,8 +327,11 @@ void drmmode_get_default_bpp(ScrnInfoPtr pScrn, drmmode_ptr drmmmode,
                              int *depth, int *bpp);
 
 void drmmode_copy_fb(ScrnInfoPtr pScrn, drmmode_ptr drmmode);
+void drmmode_copy_damage(xf86CrtcPtr crtc, PixmapPtr dst, RegionPtr damage,
+                         Bool empty);
 
-int drmmode_crtc_flip(xf86CrtcPtr crtc, uint32_t fb_id, uint32_t flags, void *data);
+int drmmode_crtc_flip(xf86CrtcPtr crtc, uint32_t fb_id, int x, int y,
+                      uint32_t flags, void *data);
 
 Bool drmmode_crtc_get_fb_id(xf86CrtcPtr crtc, uint32_t *fb_id, int *x, int *y);
 
diff --git a/hw/xfree86/drivers/modesetting/modesetting.man b/hw/xfree86/drivers/modesetting/modesetting.man
index 71790011ec93f903a7b689980578086de144e70b..9e40b04f32251ac6090d16ccbb59324272f6ae7a 100644
--- a/hw/xfree86/drivers/modesetting/modesetting.man
+++ b/hw/xfree86/drivers/modesetting/modesetting.man
@@ -109,6 +109,17 @@ When enabled, this option allows the driver to use gamma ramps with more
 entries, if supported by the kernel. By default, GAMMA_LUT will be used for
 kms drivers which are known to be safe for use of GAMMA_LUT.
 .TP
+.BI "Option \*qTearFree\*q \*q" boolean \*q
+Enable tearing prevention using the hardware page flipping mechanism.
+It allocates two extra scanout buffers for each CRTC and utilizes damage
+tracking to minimize buffer copying and skip unnecessary flips when the
+screen's contents have not changed. It works on transformed screens too, such
+as rotated and scaled CRTCs. When PageFlip is enabled, fullscreen DRI
+applications will still have the discretion to not use tearing prevention.
+.br
+The default is
+.B off.
+.TP
 .SH "SEE ALSO"
 @xservername@(@appmansuffix@), @xconfigfile@(@filemansuffix@), Xserver(@appmansuffix@),
 X(@miscmansuffix@)
diff --git a/hw/xfree86/drivers/modesetting/pageflip.c b/hw/xfree86/drivers/modesetting/pageflip.c
index 23ee95f9a68d96c037c33ce28e2afb7761c552bb..8d57047efa6823bedd5de9f930fe2aa4ef6b3ce4 100644
--- a/hw/xfree86/drivers/modesetting/pageflip.c
+++ b/hw/xfree86/drivers/modesetting/pageflip.c
@@ -35,8 +35,8 @@
  * Returns a negative value on error, 0 if there was nothing to process,
  * or 1 if we handled any events.
  */
-int
-ms_flush_drm_events(ScreenPtr screen)
+static int
+ms_flush_drm_events_timeout(ScreenPtr screen, int timeout)
 {
     ScrnInfoPtr scrn = xf86ScreenToScrn(screen);
     modesettingPtr ms = modesettingPTR(scrn);
@@ -45,7 +45,7 @@ ms_flush_drm_events(ScreenPtr screen)
     int r;
 
     do {
-            r = xserver_poll(&p, 1, 0);
+            r = xserver_poll(&p, 1, timeout);
     } while (r == -1 && (errno == EINTR || errno == EAGAIN));
 
     /* If there was an error, r will be < 0.  Return that.  If there was
@@ -63,6 +63,12 @@ ms_flush_drm_events(ScreenPtr screen)
     return 1;
 }
 
+int
+ms_flush_drm_events(ScreenPtr screen)
+{
+    return ms_flush_drm_events_timeout(screen, 0);
+}
+
 #ifdef GLAMOR_HAS_GBM
 
 /*
@@ -160,11 +166,32 @@ ms_pageflip_abort(void *data)
 }
 
 static Bool
-do_queue_flip_on_crtc(modesettingPtr ms, xf86CrtcPtr crtc,
-                      uint32_t flags, uint32_t seq)
+do_queue_flip_on_crtc(ScreenPtr screen, xf86CrtcPtr crtc, uint32_t flags,
+                      uint32_t seq, uint32_t fb_id, int x, int y)
 {
-    return drmmode_crtc_flip(crtc, ms->drmmode.fb_id, flags,
-                             (void *) (uintptr_t) seq);
+    drmmode_crtc_private_ptr drmmode_crtc = crtc->driver_private;
+    drmmode_tearfree_ptr trf = &drmmode_crtc->tearfree;
+
+    while (drmmode_crtc_flip(crtc, fb_id, x, y, flags, (void *)(long)seq)) {
+        /* We may have failed because the event queue was full.  Flush it
+         * and retry.  If there was nothing to flush, then we failed for
+         * some other reason and should just return an error.
+         */
+        if (ms_flush_drm_events(screen) <= 0) {
+            /* The failure could be caused by a pending TearFree flip, in which
+             * case we should wait until there's a new event and try again.
+             */
+            if (!trf->flip_seq || ms_flush_drm_events_timeout(screen, -1) < 0) {
+                ms_drm_abort_seq(crtc->scrn, seq);
+                return TRUE;
+            }
+        }
+
+        /* We flushed some events, so try again. */
+        xf86DrvMsg(crtc->scrn->scrnIndex, X_WARNING, "flip queue retry\n");
+    }
+
+    return FALSE;
 }
 
 enum queue_flip_status {
@@ -205,20 +232,9 @@ queue_flip_on_crtc(ScreenPtr screen, xf86CrtcPtr crtc,
     /* take a reference on flipdata for use in flip */
     flipdata->flip_count++;
 
-    while (do_queue_flip_on_crtc(ms, crtc, flags, seq)) {
-        /* We may have failed because the event queue was full.  Flush it
-         * and retry.  If there was nothing to flush, then we failed for
-         * some other reason and should just return an error.
-         */
-        if (ms_flush_drm_events(screen) <= 0) {
-            /* Aborting will also decrement flip_count and free(flip). */
-            ms_drm_abort_seq(scrn, seq);
-            return QUEUE_FLIP_DRM_FLUSH_FAILED;
-        }
-
-        /* We flushed some events, so try again. */
-        xf86DrvMsg(scrn->scrnIndex, X_WARNING, "flip queue retry\n");
-    }
+    if (do_queue_flip_on_crtc(screen, crtc, flags, seq, ms->drmmode.fb_id,
+                              crtc->x, crtc->y))
+        return QUEUE_FLIP_DRM_FLUSH_FAILED;
 
     /* The page flip succeeded. */
     return QUEUE_FLIP_SUCCESS;
@@ -465,4 +481,50 @@ error_out:
 #endif /* GLAMOR_HAS_GBM */
 }
 
+static void
+ms_tearfree_flip_abort(void *data)
+{
+    drmmode_tearfree_ptr trf = data;
+
+    trf->flip_seq = 0;
+}
+
+static void
+ms_tearfree_flip_handler(uint64_t msc, uint64_t usec, void *data)
+{
+    drmmode_tearfree_ptr trf = data;
+
+    /* Swap the buffers and complete the flip */
+    trf->back_idx ^= 1;
+    trf->flip_seq = 0;
+}
+
+Bool
+ms_do_tearfree_flip(ScreenPtr screen, xf86CrtcPtr crtc)
+{
+    drmmode_crtc_private_ptr drmmode_crtc = crtc->driver_private;
+    drmmode_tearfree_ptr trf = &drmmode_crtc->tearfree;
+    uint32_t idx = trf->back_idx, seq;
+
+    seq = ms_drm_queue_alloc(crtc, trf, ms_tearfree_flip_handler,
+                             ms_tearfree_flip_abort);
+    if (!seq)
+        goto no_flip;
+
+    /* Copy the damage to the back buffer and then flip it at the vblank */
+    drmmode_copy_damage(crtc, trf->buf[idx].px, &trf->buf[idx].dmg, TRUE);
+    if (do_queue_flip_on_crtc(screen, crtc, DRM_MODE_PAGE_FLIP_EVENT,
+                              seq, trf->buf[idx].fb_id, 0, 0))
+        goto no_flip;
+
+    trf->flip_seq = seq;
+    return FALSE;
+
+no_flip:
+    xf86DrvMsg(crtc->scrn->scrnIndex, X_WARNING,
+               "TearFree flip failed, rendering frame without TearFree\n");
+    drmmode_copy_damage(crtc, trf->buf[idx ^ 1].px,
+                        &trf->buf[idx ^ 1].dmg, FALSE);
+    return TRUE;
+}
 #endif
diff --git a/hw/xfree86/drivers/modesetting/present.c b/hw/xfree86/drivers/modesetting/present.c
index c3266d87116a8841ea4c9c302f43d8e706c427e6..642f7baaff93228b7b350b8f084c0a47d2b74655 100644
--- a/hw/xfree86/drivers/modesetting/present.c
+++ b/hw/xfree86/drivers/modesetting/present.c
@@ -318,14 +318,32 @@ ms_present_check_flip(RRCrtcPtr crtc,
     modesettingPtr ms = modesettingPTR(scrn);
 
     if (ms->drmmode.sprites_visible > 0)
-        return FALSE;
+        goto no_flip;
 
     if(!ms_present_check_unflip(crtc, window, pixmap, sync_flip, reason))
-        return FALSE;
+        goto no_flip;
 
     ms->flip_window = window;
 
     return TRUE;
+
+no_flip:
+    /* Export some info about TearFree if Present can't flip anyway */
+    if (reason && ms->drmmode.tearfree_enable) {
+        xf86CrtcPtr xf86_crtc = crtc->devPrivate;
+        drmmode_crtc_private_ptr drmmode_crtc = xf86_crtc->driver_private;
+        drmmode_tearfree_ptr trf = &drmmode_crtc->tearfree;
+
+        if (trf->buf[0].px) {
+            if (trf->flip_seq)
+                /* The driver has a TearFree flip pending */
+                *reason = PRESENT_FLIP_REASON_DRIVER_TEARFREE_FLIPPING;
+            else
+                /* The driver uses TearFree flips and there's no flip pending */
+                *reason = PRESENT_FLIP_REASON_DRIVER_TEARFREE;
+        }
+    }
+    return FALSE;
 }
 
 /*
diff --git a/hw/xfree86/drivers/modesetting/vblank.c b/hw/xfree86/drivers/modesetting/vblank.c
index ea9e7a88c5dfb55b553d66e34070f99e3fda44ac..4d250aa3480b704fdb94325885a1e453abb0c429 100644
--- a/hw/xfree86/drivers/modesetting/vblank.c
+++ b/hw/xfree86/drivers/modesetting/vblank.c
@@ -260,6 +260,51 @@ ms_get_kernel_ust_msc(xf86CrtcPtr crtc,
     }
 }
 
+static void
+ms_drm_set_seq_msc(uint32_t seq, uint64_t msc)
+{
+    struct ms_drm_queue *q;
+
+    xorg_list_for_each_entry(q, &ms_drm_queue, list) {
+        if (q->seq == seq) {
+            q->msc = msc;
+            break;
+        }
+    }
+}
+
+static void
+ms_drm_set_seq_queued(uint32_t seq, uint64_t msc)
+{
+    drmmode_crtc_private_ptr drmmode_crtc;
+    struct ms_drm_queue *q;
+
+    xorg_list_for_each_entry(q, &ms_drm_queue, list) {
+        if (q->seq == seq) {
+            drmmode_crtc = q->crtc->driver_private;
+            if (msc < drmmode_crtc->next_msc)
+                drmmode_crtc->next_msc = msc;
+            q->msc = msc;
+            q->kernel_queued = TRUE;
+            break;
+        }
+    }
+}
+
+static Bool
+ms_queue_coalesce(xf86CrtcPtr crtc, uint32_t seq, uint64_t msc)
+{
+    drmmode_crtc_private_ptr drmmode_crtc = crtc->driver_private;
+
+    /* If the next MSC is too late, then this event can't be coalesced */
+    if (msc < drmmode_crtc->next_msc)
+        return FALSE;
+
+    /* Set the target MSC on this sequence number */
+    ms_drm_set_seq_msc(seq, msc);
+    return TRUE;
+}
+
 Bool
 ms_queue_vblank(xf86CrtcPtr crtc, ms_queue_flag flags,
                 uint64_t msc, uint64_t *msc_queued, uint32_t seq)
@@ -271,6 +316,10 @@ ms_queue_vblank(xf86CrtcPtr crtc, ms_queue_flag flags,
     drmVBlank vbl;
     int ret;
 
+    /* Try coalescing this event into another to avoid event queue exhaustion */
+    if (flags == MS_QUEUE_ABSOLUTE && ms_queue_coalesce(crtc, seq, msc))
+        return TRUE;
+
     for (;;) {
         /* Queue an event at the specified sequence */
         if (ms->has_queue_sequence || !ms->tried_queue_sequence) {
@@ -287,8 +336,10 @@ ms_queue_vblank(xf86CrtcPtr crtc, ms_queue_flag flags,
             ret = drmCrtcQueueSequence(ms->fd, drmmode_crtc->mode_crtc->crtc_id,
                                        drm_flags, msc, &kernel_queued, seq);
             if (ret == 0) {
+                msc = ms_kernel_msc_to_crtc_msc(crtc, kernel_queued, TRUE);
+                ms_drm_set_seq_queued(seq, msc);
                 if (msc_queued)
-                    *msc_queued = ms_kernel_msc_to_crtc_msc(crtc, kernel_queued, TRUE);
+                    *msc_queued = msc;
                 ms->has_queue_sequence = TRUE;
                 return TRUE;
             }
@@ -310,8 +361,10 @@ ms_queue_vblank(xf86CrtcPtr crtc, ms_queue_flag flags,
         vbl.request.signal = seq;
         ret = drmWaitVBlank(ms->fd, &vbl);
         if (ret == 0) {
+            msc = ms_kernel_msc_to_crtc_msc(crtc, vbl.reply.sequence, FALSE);
+            ms_drm_set_seq_queued(seq, msc);
             if (msc_queued)
-                *msc_queued = ms_kernel_msc_to_crtc_msc(crtc, vbl.reply.sequence, FALSE);
+                *msc_queued = msc;
             return TRUE;
         }
     check:
@@ -418,13 +471,15 @@ ms_drm_queue_alloc(xf86CrtcPtr crtc,
     if (!ms_drm_seq)
         ++ms_drm_seq;
     q->seq = ms_drm_seq++;
+    q->msc = UINT64_MAX;
     q->scrn = scrn;
     q->crtc = crtc;
     q->data = data;
     q->handler = handler;
     q->abort = abort;
 
-    xorg_list_add(&q->list, &ms_drm_queue);
+    /* Keep the list formatted in ascending order of sequence number */
+    xorg_list_append(&q->list, &ms_drm_queue);
 
     return q->seq;
 }
@@ -437,9 +492,18 @@ ms_drm_queue_alloc(xf86CrtcPtr crtc,
 static void
 ms_drm_abort_one(struct ms_drm_queue *q)
 {
+    if (q->aborted)
+        return;
+
+    /* Don't remove vblank events if they were queued in the kernel */
+    if (q->kernel_queued) {
+        q->abort(q->data);
+        q->aborted = TRUE;
+    } else {
         xorg_list_del(&q->list);
         q->abort(q->data);
         free(q);
+    }
 }
 
 /**
@@ -500,18 +564,61 @@ ms_drm_sequence_handler(int fd, uint64_t frame, uint64_t ns, Bool is64bit, uint6
 {
     struct ms_drm_queue *q, *tmp;
     uint32_t seq = (uint32_t) user_data;
+    xf86CrtcPtr crtc = NULL;
+    drmmode_crtc_private_ptr drmmode_crtc;
+    uint64_t msc, next_msc = UINT64_MAX;
 
-    xorg_list_for_each_entry_safe(q, tmp, &ms_drm_queue, list) {
+    /* Handle the seq for this event first in order to get the CRTC */
+    xorg_list_for_each_entry(q, &ms_drm_queue, list) {
         if (q->seq == seq) {
-            uint64_t msc;
-
-            msc = ms_kernel_msc_to_crtc_msc(q->crtc, frame, is64bit);
+            crtc = q->crtc;
+            msc = ms_kernel_msc_to_crtc_msc(crtc, frame, is64bit);
             xorg_list_del(&q->list);
-            q->handler(msc, ns / 1000, q->data);
+            if (!q->aborted)
+                q->handler(msc, ns / 1000, q->data);
             free(q);
             break;
         }
     }
+
+    if (!crtc)
+        return;
+
+    /* Now run all of the vblank events for this CRTC with an expired MSC */
+    xorg_list_for_each_entry_safe(q, tmp, &ms_drm_queue, list) {
+        if (q->crtc == crtc && q->msc <= msc) {
+            xorg_list_del(&q->list);
+            if (!q->aborted)
+                q->handler(msc, ns / 1000, q->data);
+            free(q);
+        }
+    }
+
+    /* Find this CRTC's next queued MSC and next non-queued MSC to be handled */
+    msc = UINT64_MAX;
+    xorg_list_for_each_entry(q, &ms_drm_queue, list) {
+        if (q->crtc == crtc) {
+            if (q->kernel_queued) {
+                if (q->msc < next_msc)
+                    next_msc = q->msc;
+            } else if (q->msc < msc) {
+                msc = q->msc;
+                seq = q->seq;
+            }
+        }
+    }
+
+    /* Queue an event if the next queued MSC isn't soon enough */
+    drmmode_crtc = crtc->driver_private;
+    drmmode_crtc->next_msc = next_msc;
+    if (msc < next_msc && !ms_queue_vblank(crtc, MS_QUEUE_ABSOLUTE, msc, NULL, seq)) {
+        xf86DrvMsg(crtc->scrn->scrnIndex, X_WARNING,
+                   "failed to queue next vblank event, aborting lost events\n");
+        xorg_list_for_each_entry_safe(q, tmp, &ms_drm_queue, list) {
+            if (q->crtc == crtc && q->msc < next_msc)
+                ms_drm_abort_one(q);
+        }
+    }
 }
 
 static void
diff --git a/hw/xfree86/modes/xf86Crtc.h b/hw/xfree86/modes/xf86Crtc.h
index e36adbe0033a9afb1f1a56d6ff0934a3f22ec894..e9db8e3e53863b4b78692023a831c1dc8f8769ae 100644
--- a/hw/xfree86/modes/xf86Crtc.h
+++ b/hw/xfree86/modes/xf86Crtc.h
@@ -912,6 +912,11 @@ extern _X_EXPORT void
 extern _X_EXPORT Bool
  xf86CrtcRotate(xf86CrtcPtr crtc);
 
+extern _X_EXPORT void
+ xf86RotateCrtcRedisplay(xf86CrtcPtr crtc, PixmapPtr dst_pixmap,
+                         DrawableRec *src_drawable, RegionPtr region,
+                         Bool transform_src);
+
 /*
  * Clean up any rotation data, used when a crtc is turned off
  * as well as when rotation is disabled.
diff --git a/hw/xfree86/modes/xf86Rotate.c b/hw/xfree86/modes/xf86Rotate.c
index ea9c43c0f237acffaa808b8826d25a489d0bb48d..944a01b1c01ba9107e7e2bbcccd8bb2aa12fe29d 100644
--- a/hw/xfree86/modes/xf86Rotate.c
+++ b/hw/xfree86/modes/xf86Rotate.c
@@ -39,13 +39,13 @@
 #include "X11/extensions/dpmsconst.h"
 #include "X11/Xatom.h"
 
-static void
-xf86RotateCrtcRedisplay(xf86CrtcPtr crtc, RegionPtr region)
+void
+xf86RotateCrtcRedisplay(xf86CrtcPtr crtc, PixmapPtr dst_pixmap,
+                        DrawableRec *src_drawable, RegionPtr region,
+                        Bool transform_src)
 {
     ScrnInfoPtr scrn = crtc->scrn;
     ScreenPtr screen = scrn->pScreen;
-    WindowPtr root = screen->root;
-    PixmapPtr dst_pixmap = crtc->rotatedPixmap;
     PictFormatPtr format = PictureWindowFormat(screen->root);
     int error;
     PicturePtr src, dst;
@@ -57,7 +57,7 @@ xf86RotateCrtcRedisplay(xf86CrtcPtr crtc, RegionPtr region)
         return;
 
     src = CreatePicture(None,
-                        &root->drawable,
+                        src_drawable,
                         format,
                         CPSubwindowMode,
                         &include_inferiors, serverClient, &error);
@@ -70,9 +70,11 @@ xf86RotateCrtcRedisplay(xf86CrtcPtr crtc, RegionPtr region)
     if (!dst)
         return;
 
-    error = SetPictureTransform(src, &crtc->crtc_to_framebuffer);
-    if (error)
-        return;
+    if (transform_src) {
+        error = SetPictureTransform(src, &crtc->crtc_to_framebuffer);
+        if (error)
+            return;
+    }
     if (crtc->transform_in_use && crtc->filter)
         SetPicturePictFilter(src, crtc->filter, crtc->params, crtc->nparams);
 
@@ -205,7 +207,9 @@ xf86RotateRedisplay(ScreenPtr pScreen)
 
                 /* update damaged region */
                 if (RegionNotEmpty(&crtc_damage))
-                    xf86RotateCrtcRedisplay(crtc, &crtc_damage);
+                    xf86RotateCrtcRedisplay(crtc, crtc->rotatedPixmap,
+                                            &pScreen->root->drawable,
+                                            &crtc_damage, TRUE);
 
                 RegionUninit(&crtc_damage);
             }
diff --git a/include/pixmap.h b/include/pixmap.h
index 7144bfb30e8ba1fcd1b21e21e33db31d24460080..e251690d5620b3d2cf969a1097349624a15bd392 100644
--- a/include/pixmap.h
+++ b/include/pixmap.h
@@ -134,4 +134,9 @@ PixmapStopDirtyTracking(DrawablePtr src, PixmapPtr slave_dst);
 extern _X_EXPORT Bool
 PixmapSyncDirtyHelper(PixmapDirtyUpdatePtr dirty);
 
+extern _X_EXPORT void
+PixmapDirtyCopyArea(PixmapPtr dst, DrawablePtr src,
+                    int x, int y, int dst_x, int dst_y,
+                    RegionPtr dirty_region);
+
 #endif                          /* PIXMAP_H */
diff --git a/present/present.h b/present/present.h
index d41b36033f93fa9b8e0ff02c13f6fa9ec8524208..1d7b0ce42f192f5b0751cf31ad896d74560e207f 100644
--- a/present/present.h
+++ b/present/present.h
@@ -29,7 +29,9 @@
 
 typedef enum {
     PRESENT_FLIP_REASON_UNKNOWN,
-    PRESENT_FLIP_REASON_BUFFER_FORMAT
+    PRESENT_FLIP_REASON_BUFFER_FORMAT,
+    PRESENT_FLIP_REASON_DRIVER_TEARFREE,
+    PRESENT_FLIP_REASON_DRIVER_TEARFREE_FLIPPING
 } PresentFlipReason;
 
 typedef struct present_vblank present_vblank_rec, *present_vblank_ptr;
diff --git a/present/present_scmd.c b/present/present_scmd.c
index 239055bc10d8c934555356c4213cda37dbff711e..46fd9a1fd3341715cf3ccbe3c6fa1d1f8fca7dd6 100644
--- a/present/present_scmd.c
+++ b/present/present_scmd.c
@@ -71,6 +71,7 @@ present_check_flip(RRCrtcPtr            crtc,
     PixmapPtr                   window_pixmap;
     WindowPtr                   root = screen->root;
     present_screen_priv_ptr     screen_priv = present_screen_priv(screen);
+    PresentFlipReason           tmp_reason = PRESENT_FLIP_REASON_UNKNOWN;
 
     if (crtc) {
        screen_priv = present_screen_priv(crtc->pScreen);
@@ -91,6 +92,27 @@ present_check_flip(RRCrtcPtr            crtc,
     if (!screen_priv->info->flip)
         return FALSE;
 
+    /* Ask the driver for permission. Do this now to see if there's TearFree. */
+    if (screen_priv->info->version >= 1 && screen_priv->info->check_flip2) {
+        if (!(*screen_priv->info->check_flip2) (crtc, window, pixmap, sync_flip, &tmp_reason)) {
+            DebugPresent(("\td %08" PRIx32 " -> %08" PRIx32 "\n", window->drawable.id, pixmap ? pixmap->drawable.id : 0));
+            /* It's fine to return now unless the page flip failure reason is
+             * PRESENT_FLIP_REASON_BUFFER_FORMAT; we must only output that
+             * reason if all the other checks pass.
+             */
+            if (!reason || tmp_reason != PRESENT_FLIP_REASON_BUFFER_FORMAT) {
+                if (reason)
+                    *reason = tmp_reason;
+                return FALSE;
+            }
+        }
+    } else if (screen_priv->info->check_flip) {
+        if (!(*screen_priv->info->check_flip) (crtc, window, pixmap, sync_flip)) {
+            DebugPresent(("\td %08" PRIx32 " -> %08" PRIx32 "\n", window->drawable.id, pixmap ? pixmap->drawable.id : 0));
+            return FALSE;
+        }
+    }
+
     /* Make sure the window hasn't been redirected with Composite */
     window_pixmap = screen->GetWindowPixmap(window);
     if (window_pixmap != screen->GetScreenPixmap(screen) &&
@@ -123,17 +145,10 @@ present_check_flip(RRCrtcPtr            crtc,
         return FALSE;
     }
 
-    /* Ask the driver for permission */
-    if (screen_priv->info->version >= 1 && screen_priv->info->check_flip2) {
-        if (!(*screen_priv->info->check_flip2) (crtc, window, pixmap, sync_flip, reason)) {
-            DebugPresent(("\td %08" PRIx32 " -> %08" PRIx32 "\n", window->drawable.id, pixmap ? pixmap->drawable.id : 0));
-            return FALSE;
-        }
-    } else if (screen_priv->info->check_flip) {
-        if (!(*screen_priv->info->check_flip) (crtc, window, pixmap, sync_flip)) {
-            DebugPresent(("\td %08" PRIx32 " -> %08" PRIx32 "\n", window->drawable.id, pixmap ? pixmap->drawable.id : 0));
-            return FALSE;
-        }
+    if (tmp_reason == PRESENT_FLIP_REASON_BUFFER_FORMAT) {
+        if (reason)
+            *reason = tmp_reason;
+        return FALSE;
     }
 
     return TRUE;
@@ -456,7 +471,9 @@ present_check_flip_window (WindowPtr window)
     xorg_list_for_each_entry(vblank, &window_priv->vblank, window_list) {
         if (vblank->queued && vblank->flip && !present_check_flip(vblank->crtc, window, vblank->pixmap, vblank->sync_flip, NULL, 0, 0, &reason)) {
             vblank->flip = FALSE;
-            vblank->reason = reason;
+            /* Don't spuriously flag this as a TearFree presentation */
+            if (reason < PRESENT_FLIP_REASON_DRIVER_TEARFREE)
+                vblank->reason = reason;
             if (vblank->sync_flip)
                 vblank->exec_msc = vblank->target_msc;
         }
@@ -537,6 +554,7 @@ present_execute(present_vblank_ptr vblank, uint64_t ust, uint64_t crtc_msc)
     WindowPtr                   window = vblank->window;
     ScreenPtr                   screen = window->drawable.pScreen;
     present_screen_priv_ptr     screen_priv = present_screen_priv(screen);
+    uint64_t                    completion_msc;
     if (vblank && vblank->crtc) {
         screen_priv=present_screen_priv(vblank->crtc->pScreen);
     }
@@ -560,7 +578,9 @@ present_execute(present_vblank_ptr vblank, uint64_t ust, uint64_t crtc_msc)
     xorg_list_del(&vblank->window_list);
     vblank->queued = FALSE;
 
-    if (vblank->pixmap && vblank->window) {
+    if (vblank->pixmap && vblank->window &&
+        (vblank->reason < PRESENT_FLIP_REASON_DRIVER_TEARFREE ||
+         vblank->exec_msc != vblank->target_msc)) {
 
         if (vblank->flip) {
 
@@ -627,6 +647,30 @@ present_execute(present_vblank_ptr vblank, uint64_t ust, uint64_t crtc_msc)
 
         present_execute_copy(vblank, crtc_msc);
 
+        /* The presentation will be visible at the next vblank with TearFree, so
+         * the PresentComplete notification needs to be sent at the next vblank.
+         * If TearFree is already flipping then the presentation will be visible
+         * at the *next* next vblank.
+         */
+        completion_msc = crtc_msc + 1;
+        switch (vblank->reason) {
+        case PRESENT_FLIP_REASON_DRIVER_TEARFREE_FLIPPING:
+            if (vblank->exec_msc < crtc_msc)
+                completion_msc++;
+        case PRESENT_FLIP_REASON_DRIVER_TEARFREE:
+            if (Success == screen_priv->queue_vblank(screen,
+                                                     window,
+                                                     vblank->crtc,
+                                                     vblank->event_id,
+                                                     completion_msc)) {
+                /* Ensure present_execute_post() runs at the next MSC */
+                vblank->exec_msc = vblank->target_msc;
+                vblank->queued = TRUE;
+            }
+        default:
+            break;
+        }
+
         if (vblank->queued) {
             xorg_list_add(&vblank->event_queue, &present_exec_queue);
             xorg_list_append(&vblank->window_list,
@@ -739,6 +783,11 @@ present_scmd_pixmap(WindowPtr window,
             if (vblank->crtc != target_crtc || vblank->target_msc != target_msc)
                 continue;
 
+            /* Too late to abort now if TearFree execution already happened */
+            if (vblank->reason >= PRESENT_FLIP_REASON_DRIVER_TEARFREE &&
+                vblank->exec_msc == vblank->target_msc)
+                continue;
+
             present_vblank_scrap(vblank);
             if (vblank->flip_ready)
                 present_re_execute(vblank);
@@ -767,7 +816,12 @@ present_scmd_pixmap(WindowPtr window,
 
     vblank->event_id = ++present_scmd_event_id;
 
-    if (vblank->flip && vblank->sync_flip)
+    /* The soonest presentation is crtc_msc+2 if TearFree is already flipping */
+    if (vblank->reason == PRESENT_FLIP_REASON_DRIVER_TEARFREE_FLIPPING &&
+        !msc_is_after(vblank->exec_msc, crtc_msc + 1))
+        vblank->exec_msc -= 2;
+    else if (vblank->reason >= PRESENT_FLIP_REASON_DRIVER_TEARFREE ||
+             (vblank->flip && vblank->sync_flip))
         vblank->exec_msc--;
 
     xorg_list_append(&vblank->event_queue, &present_exec_queue);
