From: Herman Rimm <herman@rimm.ee>
Date: Sun, 8 Dec 2024 01:13:59 +0100
Subject: [PATCH] fix(imx8m): 8mq: enable imx_hab_handler

This completes af799814e2639a03b3453744f06a73e77cb66e86.

Signed-off-by: Herman Rimm <herman@rimm.ee>
---
To submit to review.trustedfirmware.org, sign in with a GitHub account.

diff --git a/plat/imx/common/include/imx_sip_svc.h b/plat/imx/common/include/imx_sip_svc.h
index 404a82959..1948bc2eb 100644
--- a/plat/imx/common/include/imx_sip_svc.h
+++ b/plat/imx/common/include/imx_sip_svc.h
@@ -88,7 +88,8 @@ int imx_src_handler(uint32_t smc_fid, u_register_t x1,
 		    u_register_t x2, u_register_t x3, void *handle);
 #endif
 
-#if defined(PLAT_imx8mm) || defined(PLAT_imx8mn) || defined(PLAT_imx8mp)
+#if defined(PLAT_imx8mm) || defined(PLAT_imx8mn) || defined(PLAT_imx8mp) || \
+	defined(PLAT_imx8mq)
 int imx_hab_handler(uint32_t smc_fid, u_register_t x1,
 		    u_register_t x2, u_register_t x3, u_register_t x4);
 #endif
diff --git a/plat/imx/imx8m/imx8mq/platform.mk b/plat/imx/imx8m/imx8mq/platform.mk
index 73179dd0c..b1b954f1d 100644
--- a/plat/imx/imx8m/imx8mq/platform.mk
+++ b/plat/imx/imx8m/imx8mq/platform.mk
@@ -30,6 +30,7 @@ BL31_SOURCES		+=	plat/imx/common/imx8_helpers.S			\
 				plat/imx/imx8m/imx8mq/imx8mq_psci.c		\
 				plat/imx/imx8m/gpc_common.c			\
 				plat/imx/imx8m/imx_aipstz.c			\
+				plat/imx/imx8m/imx_hab.c			\
 				plat/imx/imx8m/imx8m_caam.c			\
 				plat/imx/imx8m/imx8m_ccm.c			\
 				plat/imx/imx8m/imx8m_psci_common.c		\
